Release note:

LevelOne GEP-2682 (Hardware version:1)

-----------------------------------------
Firmware Version : v6.54.3857 to v6.54.3921
 
[Modification]
==============================================================
*S2025091601 - The cloud server is no longer under maintenance, disable Switch2go, TSOnline, APS for invalid functions.
 
[Fixed]
==============================================================
*Bug 24721 - Stopping a single fan's does not generate a fan fail log.
*Bug 24878 - Use API to show SYSTEM info the temperature can't show normally and model_name is incorrect，but CLI and WEB is working fine.
*Bug 24880 - Can not upgrade firmware via CLI and CLI will also show "malloc error".
*Bug 24980 - Typo in the SNMP/Trap Configuration trap detail page.
*Bug 25008 - Reload default keep IP option not work.
*Bug 24980 - Typo in the SNMP/Trap Configuration trap detail page.
*Bug 25008 - Reload default keep IP option not work.
*Bug 25182 - When VLAN trunk is configured, performing snmpwalk on the dot1dTpFdbTable OID can lead high CPU usage and SNMP polling timeout.
*Bug 25189 - When several ports are configured as VLAN trunk ports, the CPU usage spikes when they link up and start sending LLDP packets.
*Bug 25201 - The configurable range for the SNMP ICMPv6 Ping Egress Interface is inconsistent with the WEB.
 
[NOTE]
==============================================================
*To verify modifications, please follow the steps below after upgrading FW.
- Connect to console port.
- Login device via CLI.
- Type Command "reload defaults".
- Type Command "copy running-config startup-config".
- Reboot device.