Release note:

GEP-2651 (Hardware version: 1)

-----------------------------------------
Firmware Version : v6.54.3900 to v6.54.3921
 
[Modification]
==============================================================
*S2025091601 - The cloud server is no longer under maintenance, disable Switch2go, TSOnline, APS for invalid functions.
 
[Fixed]
==============================================================
*Bug 24980 - Typo in the SNMP/Trap Configuration trap detail page.
*Bug 25008 - Reload default keep IP option not work.
*Bug 25182 - When VLAN trunk is configured, performing snmpwalk on the dot1dTpFdbTable OID can lead high CPU usage and SNMP polling timeout.
*Bug 25189 - When several ports are configured as VLAN trunk ports, the CPU usage spikes when they link up and start sending LLDP packets.
*Bug 25201 - The configurable range for the SNMP ICMPv6 Ping Egress Interface is inconsistent with the WEB.
 
[NOTE]
==============================================================
*To verify modifications, please follow the steps below after upgrading FW.
- Connect to console port.
- Login device via CLI.
- Type Command "reload defaults".
- Type Command "copy running-config startup-config".
- Reboot device.


***Warning: After completing the update, empty the browser cache, otherwise the user interface may not be displayed correctly. please upgrade to it and check again, after upload firmware from v6.54.3921 remember reload to defualt configuration and save running-config to start-up config.

If anything doesn't work as expected or described, please contact our support, for Europe: service.de@ddc-group.com; rest of the world: support@level1.com; before opening a RMA claim.***