Release note:

GEP-2651 (Hardware version: 1)

-----------------------------------------
This version only apply for WEB UI upgrade. Please use to local computer is connected to the GEP-2651 Lan port through an RJ45 cable to update the firmware first. please upgrade to it and check again, after upload firmware from biild3506(v6.54.3506) remember reload to defualt configuration and save running-config to start-up config.

Release version: v6.54.3767 ~ v6.54.3900

 [Changed]
==============================================================
*PM2023011201 - Modify PD Class display method when using Non-Standard PD (ex. Legacy mode)
 
[Fixed]
==============================================================
*Bug 22773 - The poe mode set to force and then set back to enable ,the poe status and the LED shouldn't turn ON when not connect to PD.
*Bug 22833 - On web UI PoE Confiugration Help page, port configuration no need Capacitor Detection.
*Bug 22845 - Type special characters in Web PoE profile name, the field will not displayed.
*Bug 22853 - SNMPv3 communication error when system time is changed to current time.
*Bug 22845 - Type special characters in Web PoE profile name, the field will not displayed.
*Bug 23073 - LLDP Neighbor can not show ORING switch information.
*Bug 23144 - poe mode switch from force to enable that will cause short overload when using large wattage of PD.
*Bug 23271 - Unregistered IPMCv4 Flooding control should only take effect when IGMP Snooping is enabled
*Bug 23530 - Configure maximum length poe profile name via CLI, the Schedule name showing incorrect on poe config.
*Bug 23815 - NTP Time-Sync Interval failure when NTP server reconnection.
*Bug 23517 - Connect to Reach PoE5 class 4/class 8, PoE Status "Request Pwr" and "Allocate Pwr" information incorrect.
*Bug 23631 - PoE frimware version incorrect(RNU-FFFF) when use Broadcom PoE board.
*Bug 23596 - Unable delete vlan 1 from web.
*Bug 24237 - Can't use API to login device.
*Bug 24266 - The PoE Supply value will show "-111807747.4 W" in DMS Topology View.
*Bug 24721 - Stopping a single fan's does not generate a fan fail log.
*Bug 24878 - Use API to show SYSTEM info the temperature can't show normally and model_name is incorrect，but CLI and WEB is working fine.
*Bug 24880 - Can not upgrade firmware via CLI and CLI will also show "malloc error".
*Bug 24980 - Typo in the SNMP/Trap Configuration trap detail page.
*Bug 25008 - Reload default keep IP option not work.


***Warning: After completing the update, empty the browser cache, otherwise the user interface may not be displayed correctly. please upgrade to it and check again, after upload firmware from v6.54.3900 remember reload to defualt configuration and save running-config to start-up config.

If anything doesn't work as expected or described, please contact our support, for Europe: service.de@ddc-group.com; rest of the world: support@level1.com; before opening a RMA claim.***